Attachment 7 Transportation Analysis Summary
Martin Avenue (Lafayette Street to De La Cruz Boulevard

	Concept
	Martin Avenue - 64-Foot-Wide Section
	Entire Study Area

	
	Roadway Speeds
	Collision Reduction Potential
	Parking Available
	Peak Travel Time 
(min: sec)
	Annual VMT Reduction Estimate
	Substandard Level of Service

	Existing Conditions/No Build

	None
	None
	N: 84%
S: 67%
	AM: 2:35  PM: 2:33
	None
	AM: 2
PM: 3

	Four Lanes, Protected/Buffered Bikeway, Remove Parking 

	1-6 mph slower
	Negligible
	No parking on both sides
	AM: 2:35  PM: 2:33
	447
	AM: 2
PM: 3

	Four Lanes, Protected/Buffered and Parking Protected Bikeways, Remove Parking on One Side 

	1-6 mph slower
	Negligible
	N: 55%*
	AM: 2:35  PM: 2:33
	447
	AM: 2
PM: 3

	Two Lanes, Parking Protected Bike Lanes, Center Turn Lane 

	3-6 mph slower
	Yes
	Same as No Build
	AM: 2:49  PM: 2:43
	447
	AM: 4 (+2)
PM: 2 (-1)



*It is assumed that parking will be removed on the south side of Martin Avenue for the concept titled “Four Lanes, Protected/Buffered and Parking Protected Bikeways, Remove Parking on One Side”
.
